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	DC load distribution (Choose size and amount of load breaker) / 
CBI make  | for DPS 850B-48-3
	Qty

	☐	Load breaker 2 A
	

	☐	Load breaker 4 A
	

	☐	Load breaker 6 A
	

	☐	Load breaker 10 A
	

	☐	Load breaker 16 A
	

	☐	Load breaker 20 A
	

	☐	Load breaker 25 A
	

	☐	Load breaker 30 A
	

	System roof (I case of using the DC system inside an optional Wall mounting box or Supporting cabinet maybe not needed)
	

	☐	IP20 cover plates
	

	Sliding mounting rails (for easy installation)
	

	☐	Sliding rails for CellD40 power system
	

	AC input cables
	
	

	☐	Single phase CABLE 2m 
(one cable end open)
	

	☐	Single phase CABLE 2m 
(with SCHUKO connector)
	

	External alarm D-sub
	
	

	☐	External alarms are connected from D-sub connector to PSC3 controller. D-sub connector is located on back side of the system.
	

	Battery temp sensor 
	
	

	☐	Battery temp sensor 1,5m
	

	☐	Battery temp sensor 3m
	

	☐	Battery temp sensor 5m
	

	☐	Battery temp sensor 10m
	

	☐	Adapter for 2 temp sensors
	

	Battery cables
	
	

	☐	Battery cable set 1.5m 10mm2 with cable lugs (M6)
	

	☒	Battery cable set 3m 10mm2 with cable lugs (M6)
	

	Packing
	
	

	Packing material (Only needed if not installed in a wall mounting box, supporting cabinet or outdoor cabinet at Delta production)
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